# Using XML Tags to Indicate Type and Configuration of a Sentinel Protection Key

The following table describes how XML tags are used in various Licensing API methods to indicate the various types and configurations of Sentinel protection keys that are supported in Sentinel LDK.

Protection Key | Value for <type> | Value for <configuration> | Value for <key_model>
--- | --- | --- | ---
SL-Legacy | HASP-SL | <haspsl-legacy/> | SL
SL-AdminMode | HASP-SL | <haspsl-adminmode/> | Certificate
SL-UserMode | HASP-SL | <haspsl-usermode/> | Certificate
HASP HL2.16 | HASP-HL | <hasphl/> | Classic
HASP HL | HASP-HL | <hasphl/> | Basic Pro Max MaxMicro Time Master Developer Drive Net10 Net50 Net250+ NetTime10 NetTime50 NetTime250 Express For Sentinel HL (HASP or Driverless configuration) keys only: Sentinel-HL-Drive-microSD For Sentinel HL (Driverless configuration) keys only: Sentinel-HL-Max-Chip Sentinel-HL-Max-Board
Sentinel HL (HASP configuration) | HASP-HL | <sentinelhl/> <hasphl/>
Sentinel HL (Driverless configuration) | HASP-HL | <sentinelhl/> <driverless/>

## Related Topics

About XML Tags

Format XML Tags

XML Usage Samples